Hammer CornKing 10000 by Pebcak

########## Deutsch ##########
Hallo,
anbei die Stadard CornKing 6000 in der 10000er Version.

V1.2
Fahrgassenfunktion:

    - wenn nichts konfiguriert wird, arbeitet die 10.000 wie vorher: alles wird gesäht
    - optional kann die Fahrgassenfunktion konfiguriert und eingeschaltet werden, dazu vor dem Beginn des Sähens:
        + Radialmenü am Fahrzeug öffnen
        + Bis zur Saateinheit wechseln
        + Einstellung der Fahrgassenfunktion (von Oben nach Unten, im Uhrzeigersinn):
            o Einstellung des Abstandes der Fahrgassen, möglich sind Werte von 10m bis 60m in 1m Schritten per Mausklick oder per halten der Maustaste und Mausbewegung.
            o Wahl der Startseite. Wo wird am Feld gestartet? Am rechten oder linken Feldrand
            o Wahl der Spurbreite. Für welches Fahrzeug soll dessen Spurbreite berücksichtigt werden? Möglich sind hier der kleine Arion 530 oder der große Axion 940.
            o Einschalten der Fahrgassenfunktion
            o Das Radialmenü kann nun geschlossen werden.
        + Wichtig: Am Ende jeder Bahn muss die Sähmaschine angehoben werden. Denn das ist das Signal für die nächste Bahn und die neue Konfiguration wird berechnet.


Viel Spaß
Pebcak

########## English ########## (means, my english :-) I hope it is readable/understandable) 
Hello,
enclosed the standard Hammer CornKing 6000 in 10000 version.

V1.2
Tramline function

    - If you did configure anything, the sowing machine will work like before: seet the whole width
    - optional you can configure the Tramline funkction and turn it ON. To do so you have to do before start seeding:
        + Open the radial menu from your vehicle
        + Change to seeding unit
        + Configure the Tramline function (from top to down, clockwise):
            o Configure the Tramline width. Possible values are from 10m to 60m in 1m steps via mouse click or mouse hold and mouse move.
            o Choose the starting side of your field. At which side do you start? At the right or left field edge.
            o Choose the track widht. For which vehicle should the seed unit configure the tracks? Possible are for the small Arion 530 or the big Axion 940.
            o Turn the Tramline function ON.
            o Close the radial menu.
        + Note / Important: At the end of each track you have to raise the machine. Because the raising is the signal to calculate the settings for the next track.

Have fun
Pebcak