SiiNunit
{
accessory_addon_int_data : stabo.volvofh5.toyhang
{
	name: "Stabo XM 4060E"
	price: 500
	unlock: 0
	icon: "stabo"
	interior_model: "/vehicle/truck/upgrade/interior_decors/toyhang/stabo_c.pmd"
	data[]: .stabo.phys_data
}
physics_toy_data : .stabo.phys_data
{
  phys_model_look: default
  rope_material:		"/material/ropes/rope_black.mat"

  phys_model_coll:    "/vehicle/truck/upgrade/interior_decors/toyhang/cord.pmc"
  phys_model:         "/vehicle/truck/upgrade/interior_decors/toyhang/cord.pmd"
  
	toy_type:		"TT_double_rope"			# TT_rope, TT_double_rope, TT_joint, TT_joint_free
	toy_mass:		0.3				# toy mass
	linear_damping:		0.95			# damping of swinging of toy
	linear_stiffness: 	1.0

	locator_hook_offset:	(0.05892, -0.102851, -0.1122)		# offset of connection point on hook against toy locator
	rope_width:		0.004				# width of rope
	rope_length:		0.0180				# length of rope, in the case of double_rope, distance between hook and toy
	rope_hook_offset:	0.0317				# double_rope - distance between hooks, locator is in the middle
	rope_toy_offset:	0.0317				# double_rope - distance between rope tingles at toy
	rope_resolution:	8				# number of inner nodes of rope, except end nodes with anchors
	rope_linear_density:	2.0				# density, i.e. weight of rope per 1 m of length
	position_iterations:	20				# number of iterations in position solver
	node_damping:		1.0				# rope node velocity damping
  
}
}
