SiiNunit
{
accessory_addon_int_data : shape1.mercedes.ls1938_crs.antena_t
{
	name: "Antena PX Traseira"
	price: 150
	unlock: 0
	icon: "mercedes_ls1938_crs"
   
	interior_model:	"/vehicle/truck/mercedes_ls1938_crs/upgrade/antena/suporte_t.pmd"

	data[]: .bhead_dog2.phys_data
}

physics_toy_data : .bhead_dog2.phys_data
{

	phys_model:      "/vehicle/truck/mercedes_ls1938_crs/upgrade/antena/antena_t.pmd"
	phys_model_coll: "/vehicle/truck/mercedes_ls1938_crs/upgrade/antena/antena_t.pmc"
  
	toy_type:	 	"TT_joint"		# TT_rope, TT_double_rope, TT_joint
	toy_mass:	 	0.4			# toy mass
	locator_hook_offset:	(0.0f, 0.0000f, 0.000f)	# offset of connection point on hook against toy locator
  
	# definitions applied only to toys with joint
	angular_stiffness:	(100.0, 100.0)		# joint - together with angular damping influences frequency and amplitude of oscilation
	angular_damping:	(1.0, 1.5)		# joint - together with angular stiffness influences frequency and amplitude of oscilation
	angular_amplitude:	(5.0, 1.0, 0.0)	# joint - maximal deflection agains equilibrium position
}
}
