SiiNunit
{
accessory_addon_patch_data : mdfl5.mercedes.ls1938_crs.mdflpr_lft
{
	exterior_model: "/vehicle/truck/mercedes_ls1938_crs/upgrade/mudflap/mudflap_r_physic_left.pmd"
	data: .patch.phys_data
	suitable_for[]: "mudflap5.mercedes.ls1938_crs.r_mudflap"
}
physics_patch_data : .patch.phys_data
{

 	material: "/vehicle/truck/mercedes_ls1938_crs/upgrade/mudflap/textures/mudflap_scs.mat"
	area_density: 20.0
 	linear_stiffness: 1.4
	drag_coefficient: 0.3
	lift_coefficient: 0.3
	aero_model_type: "AT_two_side_lift_drag"
 	x_res: 10
	y_res: 8
	x_size: 0.360

	y_size: 0.490

}
}
