SiiNunit
{
accessory_addon_patch_data : mdfl2.mercedes.ls1938_crs.mdflpf_rght
{
	exterior_model: "/vehicle/truck/mercedes_ls1938_crs/upgrade/mudflap/mudflap_f_physic_right.pmd"
	data: .patch.phys_data
	suitable_for[]: "mudflap2.mercedes.ls1938_crs.f_mudflap"
}
physics_patch_data : .patch.phys_data
{

 	material: "/vehicle/truck/mercedes_ls1938_crs/upgrade/mudflap/textures/mudflap_cbvl.mat"
	area_density: 20.0
 	linear_stiffness: 1.4
	drag_coefficient: 0.3
	lift_coefficient: 0.3
	aero_model_type: "AT_two_side_lift_drag"
 	x_res: 10
	y_res: 8
	x_size: 0.280
	y_size: 0.340

}
}
