SiiNunit
{
accessory_addon_int_data : cb_01.9400i.cb_radio
{
	name: "CB Radio"
	price: 600
	unlock: 1
	icon: "int_9400i"
	part_type: factory

	exterior_model: "/vehicle/truck/intnational_9400/accessory/cb_radio/cb_radio.pmd"
	interior_model: "/vehicle/truck/intnational_9400/accessory/cb_radio/cb_radio_int.pmd"
	
	electric_type: vehicle_interior
	
	data[]: .cb.phys_data
}
physics_toy_data : .cb.phys_data
{
	phys_model:     "/vehicle/truck/intnational_9400/accessory/cb_radio/cb_cable_int.pmd"
	phys_model_coll:	"/vehicle/truck/intnational_9400/accessory/cb_radio/cb_cable_int.pmc"

	toy_type:	 	"TT_joint"		# TT_rope, TT_double_rope, TT_joint
	toy_mass:	 	0.4			# toy mass
	locator_hook_offset:	(0.0f, 0.0f, 0.0f)	# offset of connection point on hook against toy locator

	# definitions applied only to toys with joint
	angular_stiffness:	(300.0, 300.0)		# joint - together with angular damping influences frequency and amplitude of oscilation
	angular_damping:	(10.0, 10.0)		# joint - together with angular stiffness influences frequency and amplitude of oscilation
	angular_amplitude:	(15.0, 25.0, 0.1)	# joint - maximal deflection agains equilibrium position
}
}
