Caterpillar 1693 engines pack

About Caterpillar 1693 engine:
The Cat 1693 engine is a six-cylinder, four-stroke engine that operates on diesel fuel. 
It has a displacement of 15.8 liters, which allows for excellent power and torque output. 
The engine features a turbocharger, which helps to improve performance and efficiency by increasing the amount of air delivered to the combustion chamber.

The mod contains the following settings:
- 1693T 325HP
- 1693TA 375HP
- 1693TA 380HP
- 1693TA 425HP
- 1693TA 500HP (Tuned)

Support for the following trucks:
Freightliner:
- FLB (Harven)
- FLC (XBS)

Kenworth
- K100 (CyrusTheVirus)
- K100e (OverFloater)
- W900 (SCS)
- W900a (Bigddady)
- W900b (GTM)

Mack
- SuperLiner (CyrusTheVirus)
- R Series (Harven)

Peterbilt
- 389 (SCS)
- 389 (Viper2)
- 379 (Stas556/Fox071rus/dmitry68)
- 359 (Outlaw Transport)

Functional from version 1.56 and later for American Truck Simulator.

Note: samples similar to the engine had to be obtained because although the mod exists in version 1.31, it does not have at least the adequate exhaust and charging sounds, and it did not have the samples that are required for the FMOD sound system.

Updates:
v 1.1
- Correction of the exhaust turbo audio, according to FMod requirements.

Credits:
eelDavidGT, vsTerminus, odd_fellow