SiiNunit
{
accessory_engine_data : 38l.mazda.cosmo68.engine
{
	name: "Test ポルシェ 3.8 L Flat 6"
# テスト用 購入不可設定。
	price: 0
	unlock: 0
	info[]: "572 @@hp@@ (427@@kw@@)"
	info[]: "553 @@lb_ft@@ (750 @@nm@@)"
	info[]: "2@@dg@@250-4@@dg@@000 @@rpm@@"
	icon: "engine_01"

	part_type: aftermarket

	torque: 6300
	torque_curve[]: (800, 0.64) # 800 RPM
	torque_curve[]: (1000, 0.66) # 1000 RPM
	torque_curve[]: (1250, 0.69) # 1250 RPM
	torque_curve[]: (1500, 0.71) # 1500 RPM
	torque_curve[]: (1750, 0.73) # 1750 RPM
	torque_curve[]: (2000, 0.74) # 2000 RPM
	torque_curve[]: (2250, 0.75) # 2250 RPM
	torque_curve[]: (2500, 0.75) # 2500 RPM
	torque_curve[]: (2750, 0.75) # 2750 RPM
	torque_curve[]: (3000, 0.75) # 3000 RPM
	torque_curve[]: (3250, 0.75) # 3250 RPM
	torque_curve[]: (3500, 0.75) # 3500 RPM
	torque_curve[]: (3750, 0.75) # 3750 RPM
	torque_curve[]: (4000, 0.75) # 4000 RPM
	torque_curve[]: (4250, 0.745) # 4250 RPM
	torque_curve[]: (4500, 0.737) # 4500 RPM
	torque_curve[]: (4750, 0.73) # 4750 RPM
	torque_curve[]: (5000, 0.725) # 5000 RPM
	torque_curve[]: (5250, 0.722) # 5250 RPM
	torque_curve[]: (5500, 0.717) # 5500 RPM
	torque_curve[]: (5750, 0.71) # 5750 RPM
	torque_curve[]: (6000, 0.705) # 6000 RPM
	torque_curve[]: (6250, 0.70) # 6250 RPM
	torque_curve[]: (6500, 0.697) # 6500 RPM
	torque_curve[]: (6750, 0.692) # 6750 RPM
	torque_curve[]: (7000, 0.684) # 7000 RPM
	torque_curve[]: (7200, 0.66) # 7200 RPM

	secondary_torque: 6800 # torque x 1.26 (final drive relation)
	secondary_torque_gear_ratio: 0.79

	secondary_torque_curve[]: (1500, 0.68) # 1500 RPM
	secondary_torque_curve[]: (2000, 0.71) # 2000 RPM
	secondary_torque_curve[]: (2500, 0.72) # 2500 RPM
	secondary_torque_curve[]: (3000, 0.72) # 3000 RPM
	secondary_torque_curve[]: (3500, 0.72) # 3500 RPM
	secondary_torque_curve[]: (4000, 0.72) # 4000 RPM
	secondary_torque_curve[]: (4500, 0.71) # 4500 RPM
	secondary_torque_curve[]: (5000, 0.70) # 5000 RPM
	secondary_torque_curve[]: (5500, 0.67) # 5500 RPM
	secondary_torque_curve[]: (6000, 0.65) # 6000 RPM
	secondary_torque_curve[]: (6150, 0.64) # 6150 RPM
	secondary_torque_curve[]: (6200, 0.70) # 6200 RPM
	secondary_torque_curve[]: (6300, 0.71) # 6300 RPM
	secondary_torque_curve[]: (6500, 0.72) # 6500 RPM
	secondary_torque_curve[]: (7000, 0.74) # 7000 RPM
	secondary_torque_curve[]: (7200, 0.70) # 7200 RPM

	rpm_range_low_gear: (1750, 3500)
	rpm_range_high_gear: (1900, 3650)
	rpm_range_power: (2250, 7200)

	resistance_torque: -1

	rpm_idle: 800
	rpm_limit: 7200 # max of 3.8 L Flat 6 is 7200 RPM
	rpm_limit_neutral: 6500 # 6500 RPM max in neutral

	volume: 14
	consumption_coef: 0.30 # for actual 12.2 l/100km

@include "sound.sui"
}
}
