SiiNunit
{
physics_data: .phdata
{
	steering_speed_coef:	4.355
	steering_angle_coef:	2.010	#возврат руля на скорости
	steering_ratio_coef:	1.050    #Усилие 

	# Maximum allowed rotation of the front wheels (degrees)
	max_visual_rotation:	35

	steering_sensitivity_multiplier_0kmh:		0.480
	steering_sensitivity_multiplier_100kmh:		0.015	
	steering_sensitivity_multiplier_minimum:	0.037
	steering_sensitivity_multiplier_maximum:	0.700
	
	# maximum allowed relative angles in degrees between truck and trailer at the fifth wheel
	fifth_wheel_pitch: 26
	fifth_wheel_roll: 0

	# brake strength
	brake_torque_factor:		0.60	
	braking_curve_peak_rel:		3.9
	# where approx. the braking curve bends
	brake_characteristic_rpm:   1450.0
	
	brake_balance:1.1
	
	max_brake_temperature:500.0
	brake_cooling_rate:0.47
	brake_friction_warming_rate:0.15

	cabin_max_pitch_angle_front:6.1	
	cabin_max_pitch_angle_rear:6.10
	cabin_max_roll_angle:6.20	
	
	cabin_pitch_force_scaling_factor:1.15	
	cabin_pitch_damping_factor:1.50	
	cabin_roll_force_scaling_factor:0.98	
	cabin_roll_damping_factor:1.49
# Шасси и кабина	
	cabin_mass:800.0
	wheel_mass:1050.0 #Число выставленно в среднем.


	damping_scaling_front_factor: 0.75	
	damping_scaling_rear_factor: 0.95	
	damping_scaling_trailer_factor: 0.75
	
	sway_bar_stiffness_factor:	0.15
	
	thrust_characteristic_viscosity_factor:	0.660	
	transmission_viscosity_factor:0.100	
	transmission_viscosity_retarder_factor:	0.800	
	
	wheel_viscosity_factor:	0.100 #Вязкость колёс
	
	clutch_viscosity_factor: 0.150	
	clutch_connected_viscosity_factor:8.130
	
	torque_converter_viscosity_factor:	0.7
	torque_converter_locked_viscosity_factor:10.0
	
	manual_clutch_viscosity_factor:	 0.900
	manual_clutch_connected_viscosity_factor: 8.200
	
	inertia_scaling_const:0.85	
	transmission_rel_flywheel_inertia:0.100 #инерция трансмиссионного маховика
	air_resistance:					3.6
#жёсткость продольной
	bristle_stiffness_longitudinal_factor: 0.78	
	bristle_stiffness_lateral_factor: 0.47
#затухание	
	bristle_damping_longitudinal_factor: 0.90
	bristle_damping_lateral_factor:	0.90
#скальжение	
	slip_longitudinal_factor:0.85
	slip_lateral_factor: 0.84

}	
}

